IFC building model
Schema: "IFC2X3"
Description: "IFC2X_PLATFORM"
Time stamp: "2015-06-30T14:45:35"
Preprocessor: "Autodesk Revit MEP 2012 - 1.0"
Originating system: "20110916_2132(x64)"
Application: "Autodesk Revit MEP 2012" version "2012" identifier "Revit" by Organization "Autodesk Revit MEP 2012"

People and organizations
  Person "paulg" of Organization (no name given)
  Owner history of Person "paulg" of Organization (no name given) | application "Autodesk Revit MEP 2012" version "2012" identifier "Revit" by Organization "Autodesk Revit MEP 2012" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: MILLI SQUARE_METRE
  VOLUMEUNIT: MILLI CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT
  IFCSITE "Default" | latitude 42° 24′ 53″ | longitude -71° 15′ 29″ | elevation above sea level -0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | object type "AF6180 Unvented Water Heater (cylinder)" | names: "AF6180:AF6180 Unvented Water Heater (cylinder):AF6180 Unvented Water Heater (cylinder):2997" | property sets: PSet_Revit_Dimensions, PSet_Revit_Constraints, PSet_Revit_Phasing, Pset_Draughting, PSet_Revit_Type_Identity Data, PSet_Revit_Type_Other

Property sets
  PSet_Revit_Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Volume = 282994422.5118196 (IFCVOLUMEMEASURE) [MILLI CUBIC_METRE]
  PSet_Revit_Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Level 1" (IFCLABEL)
    Level = "Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  PSet_Revit_Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_Draughting | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Color: Red = 127 (IFCINTEGER); Green = 127 (IFCINTEGER); Blue = 127 (IFCINTEGER)
    Layername = "Generic Models" (IFCLABEL)
  Pset_Draughting | properties | on 1 object (1 IFCBUILDING)
    Color: Red = 127 (IFCINTEGER); Green = 127 (IFCINTEGER); Blue = 127 (IFCINTEGER)
    Layername = "Project Information" (IFCLABEL)
  PSet_Revit_Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Name = "Level 1" (IFCLABEL)
  PSet_Revit_Type_Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "Solid" (IFCLABEL)
    Line Weight = 1 (IFCINTEGER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  PSet_Revit_Type_Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = 0 (IFCINTEGER)
  PSet_Revit_Type_Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    Manufacturer = "Zip Heaters(UK) Ltd" (IFCLABEL)
    Model = "AF6180" (IFCLABEL)
    OmniClass Number = "" (IFCLABEL)
    OmniClass Title = "" (IFCLABEL)
    Type Comments = "Storage water heater." (IFCLABEL)
    _created by = "" (IFCLABEL)
    _distributed by = "" (IFCLABEL)
  PSet_Revit_Type_Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Barcode = 0. (IFCREAL)
    Control Handle = TRUE (IFCBOOLEAN)
    Control Handle Center = TRUE (IFCBOOLEAN)
    Low Emitting Material = TRUE (IFCBOOLEAN)
    Mixing Leaver = TRUE (IFCBOOLEAN)
    No of Holes = 0 (IFCINTEGER)
    Percentage of Recycled Content = 0. (IFCREAL)
    SerialNumber = 0. (IFCREAL)
    TagNumber = 0. (IFCREAL)
    _current revision = 1 (IFCINTEGER)
  PSet_Revit_Type_Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Clearance - Above Unit = "" (IFCLABEL)
    Clearance - Beneath Unit = "" (IFCLABEL)
    Clearance - LHS = "" (IFCLABEL)
    Clearance - RHS = "" (IFCLABEL)
    Unit Dimensions - W x D x H = "1290mm Height x 545mm Dia." (IFCLABEL)
    Weight (empty) = "45kg" (IFCLABEL)
    Weight (full) = "222kg" (IFCLABEL)
  PSet_Revit_Type_Text | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    AccessibilityPerformance = "" (IFCLABEL)
    AssetType = "Water Heater" (IFCLABEL)
    Capacity = "180 Litres" (IFCLABEL)
    Cold Water Inlet Set = "Supplied" (IFCLABEL)
    Controls = "Thermostat-adjustable to 65 deg. Expansion relief valve to 6 bar, temperature and pressure relief valve 90 deg. 'C' and 7 bar, Tundish Pressure reducing valve3 bar, Expansion vessel pre charged to 3bar." (IFCLABEL)
    CreatedBy = "" (IFCLABEL)
    CreatedOn = "" (IFCLABEL)
    Delivery (167ml cup) cups per instance = "" (IFCLABEL)
    Dual Control Thermostat = "Supplied" (IFCLABEL)
    DurationUnit = "" (IFCLABEL)
    Flow Rate = "" (IFCLABEL)
    Grommet for Solar Sensor = "" (IFCLABEL)
    InstallationDate = "" (IFCLABEL)
    Instruction Manual = "Supplied" (IFCLABEL)
    LEED Credit = "" (IFCLABEL)
    ModelNumber = "" (IFCLABEL)
    Name = "Unvented water heater" (IFCLABEL)
    Operating Pressure = "" (IFCLABEL)
    Pull out or Pull Down = "" (IFCLABEL)
    Recovery (167ml cups) cups per hour = "" (IFCLABEL)
    ReplacementCost = "" (IFCLABEL)
    Technica support /Maintenance number = "0845 6 005 005 or 0345 6 005 005" (IFCLABEL)
    Thermostat (High Limit) = "" (IFCLABEL)
    Two Port Zone Valve = "Supplied" (IFCLABEL)
    Uniclass2 = "" (IFCLABEL)
    WarrantyDescription = "" (IFCLABEL)
    WarrantyDurationParts = "" (IFCLABEL)
    WarrantyDurationUnit = "" (IFCLABEL)
    WarrantyGuarantorLabor = "" (IFCLABEL)
    WarrantyGuarantorParts = "" (IFCLABEL)
    WarrantyStartDate = "" (IFCLABEL)
    Website = "www.zipheaters.co.uk" (IFCLABEL)
  PSet_Revit_Type_Plumbing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    15x22mm Tundish = "Supplied" (IFCLABEL)
    3/4" BSP Femalex22mm Connection for Expansion Tank = "Supplied" (IFCLABEL)
    Expansion Vessel plus bracket = "Supplied" (IFCLABEL)
    Immersion Heaters (Dependant on size and Configuration). = "Supplied" (IFCLABEL)
    Indirect Heat Exchanger (energy rating) = "18.55" (IFCLABEL)
    Temperature Pressure Relief Valve = "Supplied" (IFCLABEL)
    Vent outlet connection (to Tundish outlet). = "" (IFCLABEL)
    Water inlet Connection = "22mm BSP" (IFCLABEL)
    Water inlet Pressure Min/Max = "Min = 0.15 MPa (1.5 bar) Max = 1.2 MPa (12 bar)" (IFCLABEL)
  PSet_Revit_Type_Electrical - Circuiting | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Electrical Installation connection = "To be wired to a suitably rated double pole fused spur." (IFCLABEL)
    Voltage = "230V (50~60Hz)" (IFCLABEL)
  PSet_Revit_Type_Electrical - Loads | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Power Rating = "3kW" (IFCLABEL)
  PSet_Revit_Type_Materials and Finishes | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Finish Options = "Corrosion resistant Duplex stainless steel + High performance CFC free injected polyurethane foam insulation." (IFCLABEL)