IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "HP010.ifc"
Time stamp: "2016-05-05T16:22:59"
Preprocessor: "Autodesk Revit MEP 2013"
Originating system: "20130531_2115(x64)"
Application: "Autodesk Revit MEP 2013" version "2013" identifier "Revit" by Organization "Autodesk Revit MEP 2013"

People and organizations
  Person "paulg" of Organization (no name given)
  Owner history of Person "paulg" of Organization (no name given) | application "Autodesk Revit MEP 2013" version "2013" identifier "Revit" by Organization "Autodesk Revit MEP 2013" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: MILLI SQUARE_METRE
  VOLUMEUNIT: MILLI CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT | long name "C:\Users\paulg\Desktop\On Wall Boiling Water\Hydroboil Plus_White\IFC files\HP010.ifc"
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level -0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 2 elements
          2 x IFCBUILDINGELEMENTPROXY | object type "Hydroboil Plus HP010" | names: "RFAHP010:Hydroboil Plus HP010:Hydroboil Plus HP010:4028", "RFAHP010:Hydroboil Plus HP010:Hydroboil Plus HP010:4039" | property sets: Constraints, Dimensions, Phasing, Pset_BuildingElementProxyCommon, Green Building Properties, Text

Property sets
  Constraints | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Level 1" (IFCLABEL)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = 0 (IFCINTEGER)
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Volume = 52299933.7183722 (IFCVOLUMEMEASURE) [MILLI CUBIC_METRE]
  Dimensions | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Capacity = "10.0 Litres" (IFCLABEL)
    Gross Weight = "29.5kg (When full)" (IFCLABEL)
    Net Weight = "15.0kg" (IFCLABEL)
    Overall Height = "600mm" (IFCLABEL)
    Overall Length/Depth = "244mm" (IFCLABEL)
    Overall Width = "390mm" (IFCLABEL)
    Shipping Weight = "15.0kg" (IFCLABEL)
    Tap Clearance = "200mm" (IFCLABEL)
    Unit Access Clearance Bottom = "200mm" (IFCLABEL)
    Unit Access Clearance Front = "" (IFCLABEL)
    Unit Access Clearance Left = "65mm" (IFCLABEL)
    Unit Access Clearance Rear = "" (IFCLABEL)
    Unit Access Clearance Top = "150mm" (IFCLABEL)
    Unit Access Clearance right = "20mm" (IFCLABEL)
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Phasing | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "Hydroboil Plus HP010" (IFCIDENTIFIER)
  Identity Data | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    Description = "" (IFCLABEL)
    Features = "" (IFCLABEL)
    Keynote = "" (IFCLABEL)
    Manufacturer = "Zip Industries(UK) Ltd" (IFCLABEL)
    Model = "HP010" (IFCLABEL)
    OmniClass Number = "" (IFCLABEL)
    OmniClass Title = "" (IFCLABEL)
    Product Range = "Wall Mounted" (IFCLABEL)
    Type Comments = "Boiling Water Heater (Potable)" (IFCLABEL)
    URL = "www.zipindustries.co.uk" (IFCLABEL)
    WRAS Approved = "Yes" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCLABEL)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDING)
    Building Name = "" (IFCLABEL)
    Organization Description = "" (IFCLABEL)
    Organization Name = "" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Green Building Properties | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Embodied Carbon = "" (IFCLABEL)
    Energy Technology List = "" (IFCLABEL)
    Environmental Product Declaration = "" (IFCLABEL)
    Green Guide for Specification = "" (IFCLABEL)
    Life Cycle Analysis = "" (IFCLABEL)
    Location of Manufacturer = "" (IFCLABEL)
    Material Ingredient Reporting = "" (IFCLABEL)
    Responsible Extraction of Materials = "" (IFCLABEL)
    Responsible Sourcing of Materials = "" (IFCLABEL)
  Text | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    6 Monthly Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Annually Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Bespoke Timeframe Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Daily Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Expected Life = "" (IFCLABEL)
    Maintenance Required 0-300hrs (Maintenance Tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 1001-2000hrs (Maintenance tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 2001-4000hrs (Maintenance tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 301-600hrs (Maintenance Tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 40001-8000hrs (Maintenance tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 601-1000hrs (Maintenance tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 8001-12000hrs (Maintenance required in this time frame) = "" (IFCLABEL)
    Monthly Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    O&M Manual (Manufacturer O&M Data) = "" (IFCLABEL)
    Quarterly Maintenance (or SFG20 Codes) = "In some hard water areas where mineral scale accumulation in the boilingchamber of the Zip Econoboil may become a problem, consideration should be given to the maintenance required. chamber of the Zip Econoboil may become a problem, consideration should be given to the maintenance required. necessary." (IFCLABEL)
    Warranty ID = "" (IFCLABEL)
    Weekly Maintenance (or SFG20 Codes) = "" (IFCLABEL)
  Other | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Control Thermostat Range = "68°C -- 100°C" (IFCLABEL)
    Heat Up Time = "38 minutes at 15°C and 40 minutes 10°C" (IFCLABEL)
    Max. Stored Water Temperature = "98°C" (IFCLABEL)
    Nominal Flow Rate (Boiling) = "" (IFCLABEL)
    Recovery Volume per Minute = "" (IFCLABEL)
    Single Instance Draw off Volume = "16.7 litres" (IFCLABEL)
    Volume Dispensed per hour = "30.0 litres" (IFCLABEL)
  General | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    BMS Links = "" (IFCLABEL)
    Button Interface = "Liquid crystal display panel, button controls" (IFCLABEL)
    Internal Filter (if fitted) = "N/A" (IFCLABEL)
    Programmable Function Parameters = "The Hydroboil Plus has 2 modes of operation: 1).Normal operation mode 2). Configuration mode" (IFCLABEL)
    Programmable Safety Features = "Integral Safety Lock" (IFCLABEL)
    Wireless (WIFI) = "N/A" (IFCLABEL)
  Electrical - Circuiting | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Cable Length and size (If Fitted) = "N/A" (IFCLABEL)
    Enclosure Rating = "IP23" (IFCLABEL)
    Power Rating = "3.0 kW" (IFCLABEL)
    Power Supply (Voltage) = "230v(50~60Hz)" (IFCLABEL)
    Standby Power Loss (idle mode) = "" (IFCLABEL)
    Supply Phase = "Single, A standard 13 amp double pole fused spur required" (IFCLABEL)
  Construction | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Backflow Prevention Valve = "N/A" (IFCLABEL)
    Base Unit Finish = "White enamelled steel case." (IFCLABEL)
    External Material = "Mild steel case" (IFCLABEL)
    Insulation Material = "High Density Mineral Wool" (IFCLABEL)
    Mains Pressure Limiting Valve = "If pressure is likely to exceed 0.7 MPa (7 bar), a pressure limiting valve must be fitted be installed in the cold water supply line. Zip recommends a valve rated at 3.5 bar (0.35 MPa) for this application (Zip part No. AQ3)." (IFCLABEL)
    Mains Water Connection = "1/2 inch / 12.7mm compression fitting" (IFCLABEL)
    Mains Water Pressure _ Maximum = "0.7 MPa (7 bar)." (IFCLABEL)
    Mains Water Pressure _ Minimum = "0.07 MPa (0.7 bar)" (IFCLABEL)
    Shape = "Rectangle" (IFCLABEL)
    Tank Construction Material = "Stainless Steel" (IFCLABEL)
    Tap Finish = "Red lever in display panel" (IFCLABEL)
    Type = "On The Wall Water Boiler" (IFCLABEL)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "-3000010" (IFCLABEL)
    Line Weight = 1 (IFCINTEGER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)