IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "IFCAP305.ifc"
Time stamp: "2016-07-08T09:07:06"
Preprocessor: "Autodesk Revit MEP 2013"
Originating system: "20130531_2115(x64)"
Application: "Autodesk Revit MEP 2013" version "2013" identifier "Revit" by Organization "Autodesk Revit MEP 2013"

People and organizations
  Person "paulg" of Organization (no name given)
  Owner history of Person "paulg" of Organization (no name given) | application "Autodesk Revit MEP 2013" version "2013" identifier "Revit" by Organization "Autodesk Revit MEP 2013" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: MILLI SQUARE_METRE
  VOLUMEUNIT: MILLI CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT | long name "C:\Users\paulg\Desktop\Aquapoint III\Aquapoint III Undersink\IFC files\IFCAP305.ifc"
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level -0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | object type "Zip Aquapoint III_ model_AP3/05" | names: "AP305:Zip Aquapoint III_ model_AP3/05:Zip Aquapoint III_ model_AP3/05:3179" | property sets: Constraints, Dimensions, Phasing, Pset_BuildingElementProxyCommon, Other, Identity Data

Property sets
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "-3000010" (IFCLABEL)
    Line Weight = 1 (IFCINTEGER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Level 1" (IFCLABEL)
    Level = "Level: Level 1" (IFCLABEL)
    Moves With Nearby Elements = FALSE (IFCBOOLEAN)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = 0 (IFCINTEGER)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Volume = 23455425.0254976 (IFCVOLUMEMEASURE) [MILLI CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Capacity = "6.6 L" (IFCLABEL)
    Gross Weight (When Full) = "13.5kg" (IFCLABEL)
    Net Weight = "6.2kg" (IFCLABEL)
    Overall Height = "440" (IFCLABEL)
    Overall Length/Depth/Circumference = "300" (IFCLABEL)
    Overall Width = "300" (IFCLABEL)
    Shipping Weight = "N/A" (IFCLABEL)
    Tap Clearance = "N/A" (IFCLABEL)
    Unit Access Clearance Bottom = "Pipework" (IFCLABEL)
    Unit Access Clearance Front = "N/A" (IFCLABEL)
    Unit Access Clearance Left = "N/A" (IFCLABEL)
    Unit Access Clearance Rear = "N/A" (IFCLABEL)
    Unit Access Clearance Top = "N/A" (IFCLABEL)
    Unit Access Clearance right = "N/A" (IFCLABEL)
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "Zip Aquapoint III_ model_AP3/05" (IFCIDENTIFIER)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCLABEL)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDING)
    Building Name = "" (IFCLABEL)
    Organization Description = "" (IFCLABEL)
    Organization Name = "" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    Description = "" (IFCLABEL)
    Features = "" (IFCLABEL)
    Keynote = "" (IFCLABEL)
    Manufacturer = "Zip Industries(UK) Ltd" (IFCLABEL)
    Model = "AP3/05" (IFCLABEL)
    OmniClass Number = "" (IFCLABEL)
    OmniClass Title = "" (IFCLABEL)
    Product Range = "Wall Mounted" (IFCLABEL)
    Type Comments = "Direct unvented water heater" (IFCLABEL)
    URL = "www.zipindustries.co.uk" (IFCLABEL)
    WRAS Approved = "Yes" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Control Thermostat Range = "35°C, 45°C, 55°C, 75°C" (IFCLABEL)
    Heat Up Time = "11mins" (IFCLABEL)
    Max. Stored Water Temperature = "75°C" (IFCLABEL)
    Nominal Flow Rate (Boiling) = "N/A" (IFCLABEL)
    Recovery Volume per Minute = "N/A" (IFCLABEL)
    Single Instance Draw off Volume = "N/A" (IFCLABEL)
    Volume Dispensed per hour = "N/A" (IFCLABEL)
  Text | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    6 Monthly Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Annually Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Bespoke Timeframe Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Daily Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Expected Life = "" (IFCLABEL)
    Maintenance Required 0-300hrs (Maintenance Tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 1001-2000hrs (Maintenance tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 2001-4000hrs (Maintenance tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 301-600hrs (Maintenance Tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 40001-8000hrs (Maintenance tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 601-1000hrs (Maintenance tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 8001-12000hrs (Maintenance required in this time frame) = "" (IFCLABEL)
    Monthly Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    O&M Manual (Manufacturer O&M Data) = "" (IFCLABEL)
    Quarterly Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Warranty ID = "Zip Heaters (UK) Ltd warrants that, should any part fail within 12 calendar months of installation" (IFCLABEL)
    Weekly Maintenance (or SFG20 Codes) = "" (IFCLABEL)
  Green Building Properties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Embodied Carbon = "" (IFCLABEL)
    Energy Technology List = "" (IFCLABEL)
    Environmental Product Declaration = "" (IFCLABEL)
    Green Guide for Specification = "" (IFCLABEL)
    Life Cycle Analysis = "" (IFCLABEL)
    Location of Manufacturer = "" (IFCLABEL)
    Material Ingredient Reporting = "" (IFCLABEL)
    Responsible Extraction of Materials = "" (IFCLABEL)
    Responsible Sourcing of Materials = "" (IFCLABEL)
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Backflow Prevention Valve = "N/A" (IFCLABEL)
    Base Unit Finish = "White impact resistant plastic" (IFCLABEL)
    External Material = "White impact resistant plastic" (IFCLABEL)
    Insulation Material = "High efficiency polyurethane foam insulation." (IFCLABEL)
    Mains Pressure Limiting Valve = "offered as accessory" (IFCLABEL)
    Mains Water Connection = "1/2" BSP" (IFCLABEL)
    Mains Water Pressure _ Maximum = "0.55 Mpa" (IFCLABEL)
    Mains Water Pressure _ Minimum = "N/A" (IFCLABEL)
    Shape = "Rectangular" (IFCLABEL)
    Tank Construction Material = "Glass enamelled steel sheet and pressure tested to 1.2 MPa (12 bar)." (IFCLABEL)
    Tank Thickness = "N/A" (IFCLABEL)
    Tap Finish = "N/A" (IFCLABEL)
    Type = "Direct unvented water heater" (IFCLABEL)
  Electrical - Circuiting | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Cable Length and size (If Fitted) = "1metre x 1.5sq mm" (IFCLABEL)
    Enclosure Rating = "IP24" (IFCLABEL)
    Power Rating = "2kW" (IFCLABEL)
    Power Supply (Voltage) = "230 (V~)" (IFCLABEL)
    Standby Power Loss (idle mode) = "Not Known" (IFCLABEL)
    Supply Phase = "1" (IFCLABEL)
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    BMS Links = "No" (IFCLABEL)
    Button Interface = "No" (IFCLABEL)
    Internal Filter (if fitted) = "No" (IFCLABEL)
    Programmable Function Parameters = "No" (IFCLABEL)
    Programmable Safety Features = "No" (IFCLABEL)
    Wireless (WIFI) = "No" (IFCLABEL)