IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "IFCDBX211.ifc"
Time stamp: "2016-07-21T15:14:04"
Preprocessor: "Autodesk Revit MEP 2013"
Originating system: "20130531_2115(x64)"
Application: "Autodesk Revit MEP 2013" version "2013" identifier "Revit" by Organization "Autodesk Revit MEP 2013"

People and organizations
  Person "paulg" of Organization (no name given)
  Owner history of Person "paulg" of Organization (no name given) | application "Autodesk Revit MEP 2013" version "2013" identifier "Revit" by Organization "Autodesk Revit MEP 2013" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: MILLI SQUARE_METRE
  VOLUMEUNIT: MILLI CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT | long name "C:\Users\paulg\Desktop\New Instantaneos Hot Water\DEX and DBX Models\DBX 18, 21, 24, 27 Models\IFC files\IFCDBX211.ifc"
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level -0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 1 element
          1 x IFCBUILDINGELEMENTPROXY | object type "DBX21_Electronically Controlled Instantaneous Water Heater" | names: "RFADBX21:DBX21_Electronically Controlled Instantaneous Water Heater:DBX21_Electronically Controlled Instantaneous Water Heater:3171" | property sets: Constraints, Phasing, Dimensions, Pset_BuildingElementProxyCommon, Green Building Properties, Construction

Property sets
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = 0 (IFCINTEGER)
  Constraints | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Level 1" (IFCLABEL)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Phasing | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Volume = 9338400.8808393 (IFCVOLUMEMEASURE) [MILLI CUBIC_METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Dimensions | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Capacity = "N/A" (IFCLABEL)
    Gross Weight = "3.7" (IFCLABEL)
    Net Weight = "3.3kg" (IFCLABEL)
    Overall Height = "540" (IFCLABEL)
    Overall Length/Depth = "160" (IFCLABEL)
    Overall Width = "295" (IFCLABEL)
    Recommended Installation Height (Wall mounted Units) = "N/A" (IFCLABEL)
    Shipping Weight = "Not Known" (IFCLABEL)
    Tap Clearance = "N/A" (IFCLABEL)
    Unit Access Clearance Bottom = "N/A" (IFCLABEL)
    Unit Access Clearance Front = "N/A" (IFCLABEL)
    Unit Access Clearance Left = "N/A" (IFCLABEL)
    Unit Access Clearance Rear = "N/A" (IFCLABEL)
    Unit Access Clearance Top = "N/A" (IFCLABEL)
    Unit Access Clearance right = "N/A" (IFCLABEL)
  Pset_BuildingElementProxyCommon | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Reference = "DBX21_Electronically Controlled Instantaneous Water Heater" (IFCIDENTIFIER)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCLABEL)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDING)
    Building Name = "" (IFCLABEL)
    Organization Description = "" (IFCLABEL)
    Organization Name = "" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    CE Approval = "" (IFCLABEL)
    Description = "" (IFCLABEL)
    EMC Tested and certified to BS standard = "" (IFCLABEL)
    Electrical safety tested and certified to BS standard = "" (IFCLABEL)
    Features = "" (IFCLABEL)
    Keynote = "" (IFCLABEL)
    Manufacturer = "Zip Industries(UK) Ltd" (IFCLABEL)
    Model = "DBX21" (IFCLABEL)
    OmniClass Number = "" (IFCLABEL)
    OmniClass Title = "" (IFCLABEL)
    Product Range = "Instantaneous Water Heater" (IFCLABEL)
    Type Comments = "Boiling Water Heater (Potable)" (IFCLABEL)
    URL = "www.zipindustries.co.uk" (IFCLABEL)
    WRAS Approved = "Yes" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Green Building Properties | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Embodied Carbon = "" (IFCLABEL)
    Energy Technology List = "" (IFCLABEL)
    Environmental Product Declaration = "" (IFCLABEL)
    Green Guide for Specification = "" (IFCLABEL)
    Life Cycle Analysis = "" (IFCLABEL)
    Location of Manufacturer = "" (IFCLABEL)
    Material Ingredient Reporting = "" (IFCLABEL)
    Responsible Extraction of Materials = "" (IFCLABEL)
    Responsible Sourcing of Materials = "" (IFCLABEL)
  Construction | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Backflow Prevention Valve = "Not Supplied" (IFCLABEL)
    External Material = "Hi mpact resistant White Plastic." (IFCLABEL)
    Insulation Material = "N/A" (IFCLABEL)
    Mains Pressure Limiting Valve = "Not Supplied" (IFCLABEL)
    Mains Water Connection = "1/2" BSP" (IFCLABEL)
    Mains Water Pressure (Maximum) = "The appliance must not be subject to more than 1.0 MPa (10 bar)." (IFCLABEL)
    Mains Water Pressure (Minimum) = "0.2 MPa (2 bar) is recommended for optimum performance." (IFCLABEL)
    Shape = "Rectangular" (IFCLABEL)
    Tank Construction Material = "N/A" (IFCLABEL)
    Tank Thickness = "N/A" (IFCLABEL)
    Type/Usage = "Wall Mounted Water Heater" (IFCLABEL)
  Text | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    6 Monthly Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Annually Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Bespoke Timeframe Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Daily Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Expected Life = "" (IFCLABEL)
    Maintenance Required 0-300hrs (Maintenance Tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 1001-2000hrs (Maintenance tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 2001-4000hrs (Maintenance tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 301-600hrs (Maintenance Tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 40001-8000hrs (Maintenance tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 601-1000hrs (Maintenance tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 8001-12000hrs (Maintenance required in this time frame) = "" (IFCLABEL)
    Monthly Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    O&M Manual (Manufacturer O&M Data) = "" (IFCLABEL)
    Quarterly Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Warranty ID = "12 months" (IFCLABEL)
    Weekly Maintenance (or SFG20 Codes) = "" (IFCLABEL)
  Electrical - Circuiting | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Cable Length and size (If Fitted) = "Not Fitted" (IFCLABEL)
    Enclosure Rating = "IP25" (IFCLABEL)
    Frequency = "N/A" (IFCLABEL)
    Power Rating = "21.0 kW" (IFCLABEL)
    Power Supply (Voltage) = "PE 380-400" (IFCLABEL)
    Standby Power Loss (idle mode) = "Not Known" (IFCLABEL)
    Supply Phase = "3" (IFCLABEL)
  Other | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    Control Thermostat Range = "30°C-60°C" (IFCLABEL)
    Heat Up Time = "N/A" (IFCLABEL)
    Max. Stored Water Temperature = "N/A" (IFCLABEL)
    Nominal Flow Rate @ 50°C (l/m) = "7.9" (IFCLABEL)
    Recovery Volume per Minute = "N/A" (IFCLABEL)
    Single Instance Draw off Volume = "N/A" (IFCLABEL)
    Volume Dispensed per hour = "N/A" (IFCLABEL)
  General | properties | on 1 object (1 IFCBUILDINGELEMENTPROXY)
    7 day Electronic Programming = "No" (IFCLABEL)
    BMS Links = "No" (IFCLABEL)
    Button Interface = "Yes" (IFCLABEL)
    Internal Filter (if fitted) = "No" (IFCLABEL)
    Programmable Function Parameters = "Yes" (IFCLABEL)
    Programmable Safety Features = "Yes" (IFCLABEL)
    Touch Screen Control Panel = "N0" (IFCLABEL)
    Wireless (WIFI) = "No_Radio channel of heater and remote control" (IFCLABEL)
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "-3000010" (IFCLABEL)
    Line Weight = 1 (IFCINTEGER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)