IFC building model
Schema: "IFC2X3"
Description: "ViewDefinition [CoordinationView]"
File name: "ES 4.IFC1.ifc"
Time stamp: "2016-07-25T08:51:09"
Preprocessor: "Autodesk Revit MEP 2013"
Originating system: "20130531_2115(x64)"
Application: "Autodesk Revit MEP 2013" version "2013" identifier "Revit" by Organization "Autodesk Revit MEP 2013"

People and organizations
  Person "paulg" of Organization (no name given)
  Owner history of Person "paulg" of Organization (no name given) | application "Autodesk Revit MEP 2013" version "2013" identifier "Revit" by Organization "Autodesk Revit MEP 2013" | change NOCHANGE | created 0 (1970-01-01T00:00:00Z)

Units
  LENGTHUNIT: MILLI METRE
  AREAUNIT: MILLI SQUARE_METRE
  VOLUMEUNIT: MILLI CUBIC_METRE
  PLANEANGLEUNIT: DEGREE (conversion based)
  TIMEUNIT: SECOND

Spatial structure
IFCPROJECT | long name "C:\Users\paulg\Desktop\Instantaneos Hot Water\Inline ES Models\ES 4\IFC files\ES 4.IFC1.ifc"
  IFCSITE "Default" | latitude 42° 24′ 53.508911″ | longitude -71° 15′ 29.058837″ | elevation above sea level -0.
    IFCBUILDING | postal address (none given)
      IFCBUILDINGSTOREY "Level 1" | long name "Level 1" | elevation 0.
        contains 2 elements
          2 x IFCBUILDINGELEMENTPROXY | object type "ES 4_ Electronic Instantaneous Water Heaters" | names: "ES 4.RFA:ES 4_ Electronic Instantaneous Water Heaters:ES 4_ Electronic Instantaneous Water Heaters:3963", "ES 4.RFA:ES 4_ Electronic Instantaneous Water Heaters:ES 4_ Electronic Instantaneous Water Heaters:3983" | property sets: Dimensions, Phasing, Constraints, Pset_BuildingElementProxyCommon, Construction, Electrical - Circuiting

Property sets
  Graphics | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Color = 0 (IFCINTEGER)
    Line Pattern = "-3000010" (IFCLABEL)
    Line Weight = 1 (IFCINTEGER)
    Symbol at End 1 Default = FALSE (IFCBOOLEAN)
    Symbol at End 2 Default = TRUE (IFCBOOLEAN)
  Dimensions | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Volume = 1839902.04385256 (IFCVOLUMEMEASURE) [MILLI CUBIC_METRE]
  Dimensions | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Capacity = "N/A" (IFCLABEL)
    Gross Weight = "1.5kg" (IFCLABEL)
    Net Weight = "1.3kg" (IFCLABEL)
    Overall Height = "135mm" (IFCLABEL)
    Overall Length/Depth = "87mm" (IFCLABEL)
    Overall Width = "186mm" (IFCLABEL)
    Shipping Weight = "Not Known" (IFCLABEL)
    Tap Clearance = "N/A" (IFCLABEL)
    Unit Access Clearance Bottom = "N/A" (IFCLABEL)
    Unit Access Clearance Front = "N/A" (IFCLABEL)
    Unit Access Clearance Left = "N/A" (IFCLABEL)
    Unit Access Clearance Rear = "N/A" (IFCLABEL)
    Unit Access Clearance Top = "N/A" (IFCLABEL)
    Unit Access Clearance right = "N/A" (IFCLABEL)
  Dimensions | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Computation Height = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Phasing | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Phase Created = "New Construction" (IFCLABEL)
  Constraints | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Host = "Level : Level 1" (IFCLABEL)
    Level = "Level: Level 1" (IFCLABEL)
    Offset = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation = 0. (IFCLENGTHMEASURE) [MILLI METRE]
  Constraints | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Elevation Base = 0 (IFCINTEGER)
  Pset_BuildingElementProxyCommon | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Reference = "ES 4_ Electronic Instantaneous Water Heaters" (IFCIDENTIFIER)
  Identity Data | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Assembly Code = "" (IFCLABEL)
    Assembly Description = "" (IFCLABEL)
    Description = "" (IFCLABEL)
    Features = "" (IFCLABEL)
    Keynote = "" (IFCLABEL)
    Manufacturer = "Zip Industries(UK) Ltd" (IFCLABEL)
    Model = "ES 4" (IFCLABEL)
    OmniClass Number = "" (IFCLABEL)
    OmniClass Title = "" (IFCLABEL)
    Product Range = "Instantaneous" (IFCLABEL)
    Type Comments = "Wall Mounted Water Heater" (IFCLABEL)
    URL = "www.zipindustries.co.uk" (IFCLABEL)
    WRAS Approved = "Yes" (IFCLABEL)
  Identity Data | properties | on 1 object (1 IFCBUILDINGSTOREY)
    Building Story = TRUE (IFCBOOLEAN)
    Name = "Level 1" (IFCLABEL)
    Structural = FALSE (IFCBOOLEAN)
  Identity Data | properties | on 1 object (1 IFCBUILDING)
    Building Name = "" (IFCLABEL)
    Organization Description = "" (IFCLABEL)
    Organization Name = "" (IFCLABEL)
  Pset_BuildingCommon | properties | on 1 object (1 IFCBUILDING)
    NumberOfStoreys = 1 (IFCINTEGER)
  Construction | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Backflow Prevention Valve = "Not Supplied" (IFCLABEL)
    External Material = "High Impact" (IFCLABEL)
    Insulation Material = "N/A" (IFCLABEL)
    Mains Pressure Limiting Valve = "Not Supplied" (IFCLABEL)
    Mains Water Connection = "1/2" BSP" (IFCLABEL)
    Mains Water Pressure _ Maximum = "" (IFCLABEL)
    Mains Water Pressure _ Minimum = "A minimum water pressure of 0.2 MPa (2 bar) is recommended for optimum performance." (IFCLABEL)
    Shape = "Rectangular" (IFCLABEL)
    Tank Construction Material = "N/A" (IFCLABEL)
    Tank Thickness = "N/A" (IFCLABEL)
    Tap Finish = "N/A" (IFCLABEL)
    Type = "Wall mounted instantaneous water heater" (IFCLABEL)
  Electrical - Circuiting | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Cable Length and size (If Fitted) = "Not Fitted" (IFCLABEL)
    Enclosure Rating = "IP25" (IFCLABEL)
    Power Rating ES_4 = "4.4kW" (IFCLABEL)
    Power Supply (Voltage) = "230 (v~)" (IFCLABEL)
    Standby Power Loss (idle mode) = "Not Known" (IFCLABEL)
    Supply Phase = "1" (IFCLABEL)
  Other | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Control Thermostat Range = "30°C-43°C" (IFCLABEL)
    Factory set flow rate ES_ - @3 bar l/m = "2.0" (IFCLABEL)
    Factory set flow rate ES_3 - @3 bar l/m = "2.5" (IFCLABEL)
    Factory set flow rate ES_4 - @3 bar l/m = "3.3" (IFCLABEL)
    Heat Up Time = "N/A" (IFCLABEL)
    Max. Stored Water Temperature = "N/A" (IFCLABEL)
    Recovery Volume per Minute = "N/A" (IFCLABEL)
    Single Instance Draw off Volume = "N/A" (IFCLABEL)
    Volume Dispensed per hour = "N/A" (IFCLABEL)
  Text | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    6 Monthly Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Annually Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Bespoke Timeframe Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Daily Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Expected Life = "" (IFCLABEL)
    Maintenance Required 0-300hrs (Maintenance Tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 1001-2000hrs (Maintenance tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 2001-4000hrs (Maintenance tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 301-600hrs (Maintenance Tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 40001-8000hrs (Maintenance tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 601-1000hrs (Maintenance tasks required in this time frame) = "" (IFCLABEL)
    Maintenance Required 8001-12000hrs (Maintenance required in this time frame) = "" (IFCLABEL)
    Monthly Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    O&M Manual (Manufacturer O&M Data) = "" (IFCLABEL)
    Quarterly Maintenance (or SFG20 Codes) = "" (IFCLABEL)
    Warranty ID = "12 Calender Months" (IFCLABEL)
    Weekly Maintenance (or SFG20 Codes) = "" (IFCLABEL)
  Green Building Properties | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    Embodied Carbon = "" (IFCLABEL)
    Energy Technology List = "" (IFCLABEL)
    Environmental Product Declaration = "" (IFCLABEL)
    Green Guide for Specification = "" (IFCLABEL)
    Life Cycle Analysis = "" (IFCLABEL)
    Location of Manufacturer = "" (IFCLABEL)
    Material Ingredient Reporting = "" (IFCLABEL)
    Responsible Extraction of Materials = "" (IFCLABEL)
    Responsible Sourcing of Materials = "" (IFCLABEL)
  General | properties | on 2 objects (2 IFCBUILDINGELEMENTPROXY)
    BMS Links = "No" (IFCLABEL)
    Button Interface = "No" (IFCLABEL)
    Internal Filter (if fitted) = "No" (IFCLABEL)
    Programmable Function Parameters = "No" (IFCLABEL)
    Programmable Safety Features = "No" (IFCLABEL)
    Wireless (WIFI) = "No" (IFCLABEL)